

**实验一**

1.展示图





2.运行代码

/\* USER CODE BEGIN Header \*/

/\*\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* @file : main.c

\* @brief : Main program body

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\* @attention

\*

\* <h2><center>&copy; Copyright (c) 2020 STMicroelectronics.

\* All rights reserved.</center></h2>

\*

\* This software component is licensed by ST under BSD 3-Clause license,

\* the "License"; You may not use this file except in compliance with the

\* License. You may obtain a copy of the License at:

\* opensource.org/licenses/BSD-3-Clause

\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*/

/\* USER CODE END Header \*/

/\* Includes ------------------------------------------------------------------\*/

#include "main.h"

#include "gpio.h"

/\* Private includes ----------------------------------------------------------\*/

/\* USER CODE BEGIN Includes \*/

/\* USER CODE END Includes \*/

/\* Private typedef -----------------------------------------------------------\*/

/\* USER CODE BEGIN PTD \*/

/\* USER CODE END PTD \*/

/\* Private define ------------------------------------------------------------\*/

/\* USER CODE BEGIN PD \*/

/\* USER CODE END PD \*/

/\* Private macro -------------------------------------------------------------\*/

/\* USER CODE BEGIN PM \*/

/\* USER CODE END PM \*/

/\* Private variables ---------------------------------------------------------\*/

/\* USER CODE BEGIN PV \*/

/\* USER CODE END PV \*/

/\* Private function prototypes -----------------------------------------------\*/

void SystemClock\_Config(void);

/\* USER CODE BEGIN PFP \*/

/\* USER CODE END PFP \*/

/\* Private user code ---------------------------------------------------------\*/

/\* USER CODE BEGIN 0 \*/

/\* USER CODE END 0 \*/

/\*\*

\* @brief The application entry point.

\* @retval int

\*/

int main(void)

{

/\* USER CODE BEGIN 1 \*/

/\* USER CODE END 1 \*/

/\* MCU Configuration--------------------------------------------------------\*/

/\* Reset of all peripherals, Initializes the Flash interface and the Systick. \*/

HAL\_Init();

/\* USER CODE BEGIN Init \*/

/\* USER CODE END Init \*/

/\* Configure the system clock \*/

SystemClock\_Config();

/\* USER CODE BEGIN SysInit \*/

/\* USER CODE END SysInit \*/

/\* Initialize all configured peripherals \*/

MX\_GPIO\_Init();

/\* USER CODE BEGIN 2 \*/

/\* USER CODE END 2 \*/

/\* Infinite loop \*/

/\* USER CODE BEGIN WHILE \*/

while (1)

{

/\* USER CODE END WHILE \*/

/\* USER CODE BEGIN 3 \*/

HAL\_Delay(200);

HAL\_GPIO\_TogglePin(GPIOC, GPIO\_PIN\_13);

}

/\* USER CODE END 3 \*/

}

/\*\*

\* @brief System Clock Configuration

\* @retval None

\*/

void SystemClock\_Config(void)

{

RCC\_OscInitTypeDef RCC\_OscInitStruct = {0};

RCC\_ClkInitTypeDef RCC\_ClkInitStruct = {0};

/\*\* Initializes the CPU, AHB and APB busses clocks

\*/

RCC\_OscInitStruct.OscillatorType = RCC\_OSCILLATORTYPE\_HSE;

RCC\_OscInitStruct.HSEState = RCC\_HSE\_ON;

RCC\_OscInitStruct.PLL.PLLState = RCC\_PLL\_ON;

RCC\_OscInitStruct.PLL.PLLSource = RCC\_PLLSOURCE\_HSE;

RCC\_OscInitStruct.PLL.PLLM = 1;

RCC\_OscInitStruct.PLL.PLLN = 20;

RCC\_OscInitStruct.PLL.PLLP = RCC\_PLLP\_DIV7;

RCC\_OscInitStruct.PLL.PLLQ = RCC\_PLLQ\_DIV2;

RCC\_OscInitStruct.PLL.PLLR = RCC\_PLLR\_DIV2;

if (HAL\_RCC\_OscConfig(&RCC\_OscInitStruct) != HAL\_OK)

{

Error\_Handler();

}

/\*\* Initializes the CPU, AHB and APB busses clocks

\*/

RCC\_ClkInitStruct.ClockType = RCC\_CLOCKTYPE\_HCLK|RCC\_CLOCKTYPE\_SYSCLK

|RCC\_CLOCKTYPE\_PCLK1|RCC\_CLOCKTYPE\_PCLK2;

RCC\_ClkInitStruct.SYSCLKSource = RCC\_SYSCLKSOURCE\_PLLCLK;

RCC\_ClkInitStruct.AHBCLKDivider = RCC\_SYSCLK\_DIV1;

RCC\_ClkInitStruct.APB1CLKDivider = RCC\_HCLK\_DIV1;

RCC\_ClkInitStruct.APB2CLKDivider = RCC\_HCLK\_DIV1;

if (HAL\_RCC\_ClockConfig(&RCC\_ClkInitStruct, FLASH\_LATENCY\_4) != HAL\_OK)

{

Error\_Handler();

}

/\*\* Configure the main internal regulator output voltage

\*/

if (HAL\_PWREx\_ControlVoltageScaling(PWR\_REGULATOR\_VOLTAGE\_SCALE1) != HAL\_OK)

{

Error\_Handler();

}

}

/\* USER CODE BEGIN 4 \*/

/\* USER CODE END 4 \*/

/\*\*

\* @brief This function is executed in case of error occurrence.

\* @retval None

\*/

void Error\_Handler(void)

{

/\* USER CODE BEGIN Error\_Handler\_Debug \*/

/\* User can add his own implementation to report the HAL error return state \*/

/\* USER CODE END Error\_Handler\_Debug \*/

}

#ifdef USE\_FULL\_ASSERT

/\*\*

\* @brief Reports the name of the source file and the source line number

\* where the assert\_param error has occurred.

\* @param file: pointer to the source file name

\* @param line: assert\_param error line source number

\* @retval None

\*/

void assert\_failed(char \*file, uint32\_t line)

{

/\* USER CODE BEGIN 6 \*/

/\* User can add his own implementation to report the file name and line number,

tex: printf("Wrong parameters value: file %s on line %d\r\n", file, line) \*/

/\* USER CODE END 6 \*/

}

#endif /\* USE\_FULL\_ASSERT \*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* (C) COPYRIGHT STMicroelectronics \*\*\*\*\*END OF FILE\*\*\*\*/

3.LED灯效果图

